|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Test case Id | Bug Line No. | Bug Description | Expected Result | Observed Result |
| 19 | 95 | The value with which Interstatus is masked is changed to 0xffff | No assertion should fail | Package- Intermittent Failure assertion failed |
| 20 | 104 | Mode value either can be 11 or 44 but changed to and. | All Absolute Intermittent Fails assertions should fail. | All of the Absolute Intermittent and Permanent assertions failed |